GOLDSTAR ELECTRONICS INTERNATIONAL, INC.

IODE-3290U
FUNCTION
Jumper Location
Pin Settings (Closed)

Floppy drive Enabled
2
12

Floppy drive Disabled
2
23

Pinter port Enabled
3
12

Pinter port Disabled
3
23

Serial port 1 Enabled
4
12

Serial port 1 Disabled
4
23

Serial port 2 Enabled
5
23

Serial port 2 Disabled
5
12

Game prot Enabled
6
12

Game prot Disabled
6
23

Hard drive Enabled
7
12

Hard drive Disabled
7
23

Floppy drive address 3F1
8
12

Floppy drive address 371
8
23

Pinter port address 378
9
12

Pinter port address 278
9
23

Serial port 1 address 3F8
10
12

Serial port 1 address 3E8
10
23

Serial port 2 address 2F8
11
12

Serial port 2 address 2E8
11
23

Hard drive address 1F0
12
12

Hard drive address 170
12
23

Printer port IRQ 7
15
12

Printer port IRQ 5
15
23

Serial Port 1 IRQ 4
16
12

Serial Port 1 IRQ 3
16
23

Serial Port 2 IRQ 3
17
12

Serial Port 2 IRQ 4
17
23





